
How to backup or restore the netis router’s configuration

Sometimes we may need to upgrade the router to another firmware version if the current firmware version can no longer satisfies your requirement. The router’s configuration will be lost, when you upgrade the new firmware. So you can backup the router’s configuration before you upgrade the new firmware.


The Physical connection is as below:

Step 1. Open the web browser and type the IP address of the router (default:192.168.1.1) into the address bar, then press Enter.



Note: The address 192.168.1.1 is NOT on the Internet. The web-based configuration page is built into the router.

Step 2. Click **System Tools**🡪**Backup & Restore** button.

Step 3. Click the **Backup** button to save all configuration settings to your local computer as a file.

* To restore the Router's configuration, follow these instructions:

1. Click the **Browse** button to find the configuration file which you want to restore.
2. Click the **Restore** button to update the configuration with the file whose path is the one you have input or selected in the blank.

Note: The current configuration will be covered with the uploading configuration file. Wrong process will lead the device unmanaged. The restoring process lasts for 20 seconds and the Router will restart automatically then. Keep the power of the Router on during the process, in case of any damage.